**KENYA BUREAU OF STANDARDS**

**ADOPTION PROPOSAL**

|  |  |  |
| --- | --- | --- |
| **Document Type:** | **Adoption proposal** | |
| **Dates:** | Circulation date | Closing date |
| 20/02/2019 | 22/03/2019 |
| **TC Secretary** | **This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Daniel Kitui kituid@kebs.org** | |

The Kenya Bureau of Standards intends to adopt the International Standards as detailed here below

1. **Number:** IEC 60335-1:2010+AMD1:2013+AMD2:2016

**Title:** Household and similar electrical appliances - Safety - Part 1: General requirements

**Scope:**

This International Standard deals with the safety of electrical appliances for household and similar purposes, their rated voltage being not more than 250 V for single-phase appliances and 480 V for other appliances.

**Online Preview**:

1. **Number:** IEC 60335-2-23: 2016

**Title:** Household and similar electrical appliances - Safety - Part 2-23: Particular requirements for appliances for skin or hair care

**Scope:** This part of IEC 60335 deals with the safety of electric appliances for the care of skin or hair of persons or animals and intended for household and similar purposes, their rated voltage being not more than 250 V.

**Online Preview**: <https://webstore.iec.ch/preview/info_iec60335-2-23%7Bed6.0.RLV%7Den.pdf>

1. **Number:** IEC 60335-2-8:2012+AMD1:2015+AMD2:2018

**Title:** Household and similar electrical appliances - Safety - Part 2-8: Particular requirements for shavers, hair clippers and similar appliances

**Scope:** This International Standard deals with the safety of electric shavers, hair clippers and similar

appliances intended for household and similar purposes, their rated voltage being not more

than 250 V.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-8%7Bed6.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-8%7Bed6.2%7Db.pdf)

1. **Number:** IEC 60335-2-26:2002+AMD1:2008

**Title:** Household and similar electrical appliances - Safety - Part 2-26: Particular requirements for clocks

**Scope:** This International Standard deals with the safety of electric clocks having a rated voltage not

more than 250 V.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-26%7Bed4.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-26%7Bed4.1%7Db.pdf)

1. **Number:** IEC 60335-2-14:2016

**Title:** Household and similar electrical appliances - Safety - Part 2-14: Particular requirements for kitchen machines

**Scope:** This part of IEC 60335 deals with the safety of electric kitchen machines for household and

similar purposes, their rated voltage being not more than 250 V.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-14%7Bed6.0.RLV%7Den.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-14%7Bed6.0.RLV%7Den.pdf)

1. **Number:** IEC 60335-2-80: 2015

**Title:** Household and similar electrical appliances – Safety – Part 2-80: Particular requirements for fans

**Scope:** This International Standard deals with the safety of electric fans for household and similar

purposes, their rated voltage being not more than 250 V for single-phase appliances and

480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-80%7Bed3.0.RLV%7Den.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-80%7Bed3.0.RLV%7Den.pdf)

1. **Number:** IEC 60335-2-13:2009+AMD1:2016

**Title:** Household and similar electrical appliances - Safety - Part 2-13: Particular requirements for deep fat fryers, frying pans and similar appliances

**Scope:** This International Standard deals with the safety of electric deep fat fryers having a

recommended maximum quantity of oil not exceeding 5 l, frying pans, woks and other

appliances in which oil is used for cooking, and intended for household use and similar use,

their rated voltage being not more than 250 V.

Appliances intended for normal household and similar use and that may also be used by

laymen in shops, in light industry and on farms are within the scope of this standard.

However, if the appliance is intended to be used professionally to process food for

commercial consumption, the appliance is not considered to be for household and similar use

only.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-13%7Bed6.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-13%7Bed6.1%7Db.pdf)

1. **Number:** IEC 60335-2-28:2002+AMD1:2008

**Title:** Household and similar electrical appliances - Safety - Part 2-28: Particular requirements for sewing machines

**Scope:** This International Standard deals with the safety of electric sewing machines for household

and similar use, their rated voltage being not more than 250 V for single-phase appliances

and 480 V for other appliances.

Overlock machines and electrical sets are within the scope of the standard.

Appliances not intended for normal household use, but that nevertheless may be a source of

danger to the public, such as sewing machines intended to be used by laymen in shops and in

light industry, are within the scope of this standard.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-28%7Bed4.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-28%7Bed4.1%7Db.pdf)

1. **Number:** IEC 60335-2-38: 2017

**Title:** Household and similar electrical appliances - Safety - Part 2-38: Particular requirements for commercial electric griddles and griddle grills.

**Scope:** This International Standard deals with the safety of electrically operated commercial griddles

and griddle grills not intended for household use and similar use, their rated voltage being

not more than 250 V for single-phase appliances connected between one phase and neutral

and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-38%7Bed5.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-38%7Bed5.2%7Db.pdf)

1. **Number:** IEC 60335-2-42:2002+AMD1:2008+AMD2:2017

**Title:** Household and similar electrical appliances - Safety - Part 2-42: Particular requirements for commercial electric forced convection ovens, steam cookers and steam-convection ovens.

**Scope:** This International Standard deals with the safety of electrically operated commercial forced

convection ovens, steam cookers, steam-convection ovens and, exclusive of any other

use, steam generators, not intended for household and similar use, their rated voltage being

not more than 250 V for single-phase appliances connected between one phase and neutral

and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-42%7Bed5.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-42%7Bed5.2%7Db.pdf)

1. **Number:** IEC 60335-2-2:2009+AMD1:2012+AMD2:2016

**Title:** Household and similar electrical appliances – Safety –Part 2-2: Particular requirements for vacuum cleaners and water-suction cleaning appliances

**Scope:** This International Standard deals with the safety of electric vacuum cleaners and water suction cleaning appliances for household and similar purposes, including vacuum cleaners for animal grooming, their rated voltage being not more than 250 V. It also applies to centrally-sited vacuum cleaners and automatic battery-powered cleaners. This standard also applies to motorized cleaning heads and current-carrying hoses associated with a particular vacuum cleaner.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-2%7Bed6.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-2%7Bed6.2%7Db.pdf)

1. **Number:** IEC 60335-2-30:2009+AMD1:2016

**Title:** Household and similar electrical appliances - Safety -Part 2-30: Particular requirements for room heaters

**Scope:** This International Standard deals with the safety of electric room heaters for household and

similar purposes, their rated voltage being not more than 250 V for single-phase appliances

and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-30%7Bed5.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-30%7Bed5.1%7Db.pdf)

1. **Number:** IEC 60335-2-5:2012+AMD1:2018

**Title:** Household and similar electrical appliances - Safety - Part 2-5: Particular requirements for dishwashers

**Scope:** This International Standard deals with the safety of electric dishwashers for household and

similar purposes that are intended for washing and rinsing dishes, cutlery and other utensils,

their rated voltage being not more than 250 V for single-phase appliances and 480 V for

other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-5%7Bed6.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-5%7Bed6.1%7Db.pdf)

1. **Number:** IEC 60335-2-7:2008+AMD1:2011+AMD2:2016

**Title:** Household and similar electrical appliances - Safety - Part 2-7: Particular requirements for washing machines

**Scope:** This International Standard deals with the safety of electric washing machines for household

and similar use, that are intended for washing clothes and textiles, their rated voltage being

not more than 250 V for single-phase appliances and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-7%7Bed7.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-7%7Bed7.2%7Db.pdf)

1. **Number:** IEC 60335-2-11:2008+AMD1:2012+AMD2:2015

**Title:** Household and similar electrical appliances - Safety - Part 2-11: Particular requirements for tumble dryers

**Scope:** This International Standard deals with the safety of electric tumble dryers intended for

household and similar purposes, their rated voltage being not more than 250 V for singlephase appliances and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-11%7Bed7.2%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-11%7Bed7.2%7Db.pdf)

1. **Number:** IEC 60335-2-13:2009+AMD1:2016

**Title:** Household and similar electrical appliances - Safety - Part 2-13: Particular requirements for deep fat fryers, frying pans and similar appliances.

**Scope:** This International Standard deals with the safety of electric deep fat fryers having a

recommended maximum quantity of oil not exceeding 5 l, frying pans, woks and other

appliances in which oil is used for cooking, and intended for household use and similar use,

their rated voltage being not more than 250 V.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-13%7Bed6.1%7Db.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-13%7Bed6.1%7Db.pdf)

1. **Number:** IEC 60335-2-36:2017

**Title:** Household and similar electrical appliances - Safety - Part 2-36: Particular requirements for commercial electric cooking ranges, ovens, hobs and hob elements

**Scope:** This International Standard deals with the safety of electrically operated commercial cooking

and baking ranges, ovens, hobs, hob elements and similar appliances not intended for

household and similar use, their rated voltage being not more than 250 V for single-phase

appliances connected between one phase and neutral and 480 V for other appliances.

**Online Preview:** [**https://webstore.iec.ch/preview/info\_iec60335-2-36%7Bed6.0%7Den.pdf**](https://webstore.iec.ch/preview/info_iec60335-2-36%7Bed6.0%7Den.pdf)

We are therefore seeking views from potential users in respect of the same. The Standards are available at the Kenya Bureau of Standards Information Centre and a preview via the links on the individual standards.

Please tick and fill your preference of the listed option. (If the spaces provided are not enough, please attach a separate sheet of paper).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Standard | Adoption Accepted | Adoption not Acceptable | Recommendation |
| 1. | IEC 60335-1:2010+AMD1:2013+AMD2:2016 |  |  |  |
| 2. | IEC 60335-2-23: 2016 |  |  |  |
| 3. | IEC 60335-2-8:2012+AMD1:2015+AMD2:2018 |  |  |  |
| 4. | IEC 60335-2-26:2002+AMD1:2008 |  |  |  |
| 5. | IEC 60335-2-14:2016 |  |  |  |
| 6. | IEC 60335-2-80: 2015 |  |  |  |
| 7. | IEC 60335-2-13:2009+AMD1:2016 |  |  |  |
| 8. | IEC 60335-2-28:2002+AMD1:2008 |  |  |  |
| 9. | IEC 60335-2-38: 2017 |  |  |  |
| 10. | IEC 60335-2-42:2002+AMD1:2008+AMD2:2017 |  |  |  |
| 11. | IEC 60335-2-2:2009+AMD1:2012+AMD2:2016 |  |  |  |
| 12. | IEC 60335-2-30:2009+AMD1:2016 |  |  |  |
| 13. | IEC 60335-2-5:2012+AMD1:2018 |  |  |  |
| 14. | IEC 60335-2-7:2008+AMD1:2011+AMD2:2016 |  |  |  |
| 15. | IEC 60335-2-11:2008+AMD1:2012+AMD2:2015 |  |  |  |
| 16. | IEC 60335-2-13:2009+AMD1:2016 |  |  |  |
| 17. | IEC 60335-2-36:2017 |  |  |  |
|  |  |  |  |  |

Name and signature (of respondent) ………………………………………… Position…………………

Signature: …………………………………………………….

On behalf of: (Name of organization)

Date:

**NOTE:** Absence of any reply or comments shall be deemed to be an acceptance of the proposal for confirmation and **shall constitute an approval vote**.