ADOPTION PROPOSAL FORM

**CPR183/F12**

**KENYA BUREAU OF STANDARDS**

|  |  |  |
| --- | --- | --- |
| **Title:** | **IEC/IEEE 62209-1528:2020**, Measurement procedure for the assessment of specific absorption rate of human exposure to radio frequency fields from hand-held and body-worn wireless communication devices - Human models, instrumentation and procedures (Frequency range of 4 MHz to 10 GHz) | |
| **Document Type:** | **Adoption proposal** | |
| **Dates:** | Circulation date | Closing date |
| 2022-10-17 | 2022-11-17 |
| **TC Secretary** | **This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Zacheus Mwatha (zimwatha@kebs.org)** | |

The Kenya Bureau of Standards intends to adopt the International Standards as detailed here below

**Number:** **IEC/IEEE 62209-1528:2020 (**[info\_iecieee62209-1528{ed1.0}b.pdf](https://webstore.iec.ch/preview/info_iecieee62209-1528%7Bed1.0%7Db.pdf))

**Title:** Measurement procedure for the assessment of specific absorption rate of human exposure to radio frequency fields from hand-held and body-worn wireless communication devices - Human models, instrumentation and procedures (Frequency range of 4 MHz to 10 GHz)

**Scope**: IEC/IEEE 62209-1528:2020 specifies protocols and test procedures for the reproducible and repeatable measurement of the conservative exposure peak spatial average SAR (psSAR) induced inside a simplified model of the head and the body by radio-frequency (RF) transmitting devices, with a defined measurement uncertainty. These protocols and procedures apply to a significant majority of the population, including children, during the use of hand-held and body-worn wireless communication devices. These devices include single or multiple transmitters or antennas, and are operated with their radiating structure(s) at distances up to 200 mm from a human head or body. This document is employed to evaluate SAR compliance of different types of wireless communication devices used next to the ear, in front of the face, mounted on the body, operating in conjunction with other RF-transmitting, non-transmitting devices or accessories (e.g. belt-clips), or embedded in garments. The applicable frequency range is from 4 MHz to 10 GHz. Devices operating in the applicable frequency range can be tested using the phantoms and other requirements defined in this document.

The device categories covered include, but are not limited to, mobile telephones, cordless microphones, and radio transmitters in personal, desktop and laptop computers, for multi band operations using single or multiple antennas, including push-to-talk devices. This document can also be applied for wireless power transfer devices operating above 4 MHz.

This document does not apply to implanted medical devices.

This standard withdraws and replaces KS IEC 62209-1:2016 and KS IEC 62209-2:2010

We are therefore seeking views from potential users in respect of the same. The Standard is available at the Kenya Bureau of Standards Information Centre. Please tick and fill your preference of the listed option. (If the spaces provided are not enough, please use the attached template).

Adoption acceptable as presented

...............................................................................................................................

...............................................................................................................................

Adoption proposal not acceptable because of the reason(s) below

...............................................................................................................................

...............................................................................................................................

Our Recommendations are as follows

...............................................................................................................................

...............................................................................................................................

Name and Signature (of respondent): ................................................

Position (of respondent): .....................................

On behalf of ......................................................................................... (Name of organization)

Date .........................................................................

**NOTE:** Absence of any reply or comments shall be deemed to be an acceptance of the proposal for adoption and **shall constitute an approval vote**.

**COMMENTS**

**CPR 183/F12**

|  |  |  |
| --- | --- | --- |
| **Title:** | **IEC/IEEE 62209-1528:2020,** Measurement procedure for the assessment of specific absorption rate of human exposure to radio frequency fields from hand-held and body-worn wireless communication devices - Human models, instrumentation and procedures (Frequency range of 4 MHz to 10 GHz) | |
| **Document Type:** | Adoption Proposal | |
| **Dates:** | Circulation date | Closing date |
| 2022-10-17 | 2022-11-17 |
| **Recipient** | **This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Zacheus Mwatha (zimwatha@kebs.org)** | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Organization | Clause | Paragraph/ Figure/Table | Type of comment (General/Technical /Editorial) | COMMENTS | Proposed Change | TC Observation(s) |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |