**STA/SD/OP/05/F1**

**KENYA BUREAU OF STANDARDS**

**CONFIRMATION PROPOSAL FORM**

|  |  |  |
| --- | --- | --- |
| **Document Type:** | **Confirmation proposal** | |
| **Dates:** | Circulation date | Closing date |
| 2019-04-25 | 2019-05-16 |
| **TC Secretary** | **This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Daniel Kitui (kituid@kebs.org)** | |

The Kenya Bureau of Standards intends to confirm the Kenya Standards as detailed in the attached list of Kenya Standards for Systematic Review.

We are therefore seeking views from potential users in respect of relevance and effectiveness of the attached standard(s) in addressing current market needs, regulatory needs and scientific and technological development.

The Standard is available at the Kenya Bureau of Standards Information Resource Centre. Please tick (mark) and fill your preference of the listed option. (If the spaces provided are not enough, please attach a separate sheet of paper).

1. **KS Number and title:** KS 1111-39:2005 Safety of household and similar electrical appliances - Part 39: Particular requirements for humidifiers intended for use with heating, ventilation, or air-conditioning systems

**Scope:** This International Standard deals with the safety of electric humidifiers intended for use with heating, ventilation, or air-conditioning systems in household, commercial, and light industrial applications (and may include large stand-alone commercial equipment) which operate according to the evaporative or atomization system, water-injection, steam and the like, their maximum rated voltage being not more than 250 V for single-phase appliances and 600 V for all other appliances.

1. **KS Number and title:** KS 1111-42:2005 Safety of household and similar electrical appliances - Part 42: Particular requirements for pedestrian-controlled mains-operated lawn scarifiers and aerators

**Scope:** This International Standard deals with the safety of pedestrian-controlled mains-operated electrical lawn scarifiers and aerators with rotating cutters for regenerating lawns by, for instance, combing out grass thatch and moss, or by cutting vertically into the lawn face. These scarifiers are designed primarily for use at and around the home or for similar purposes, their rated voltage being not more than 250 V single phase.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Standard | Adoption Accepted | Adoption not Acceptable | Recommendation |
| 1. | KS 1111-39:2005 |  |  |  |
| 2. | KS 1111-42:2005 |  |  |  |

Our justification for the objection of the proposed confirmation is as follows (cite specific clauses and wording preferred):

………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………

Note: Absence of sustainable technical justifications in support of the objection shall render the objection unviable.

Name and (of respondent)……………………………………………… Position…………………

Signature: …………………………………………………….

On behalf of: (Name of organization)

Date:

**NOTE:** Absence of any reply or comments shall be deemed to be an acceptance of the proposal for confirmation and **shall constitute an approval vote**.